Register description

# Registers

|  |  |  |
| --- | --- | --- |
| Address | Register Name | Description |
| 0x00 | reg0 | write something useful for reg0 |
| 0x01 | reg1 | write something useful for reg0 |
| 0x02 | reg2 | write something useful for reg0 |
| 0x03 | reg3 | write something useful for reg3 |
| 0x04 | reg4 | reg4 is a very useful register. It can take down the moon when configured correctly. |
| 0x05 | reg5 | reg5 is as useful as reg4 but without a reset value defined. |
| 0x06 | reg6 | reg6 is a read only register. |
| 0x07 | reg7 | write something useful for reg7 |

# reg0

Name

reg0

Address

0x0

Reset Value

0x00000000

Access

read-write

Description

write something useful for reg0

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:24] | byte3 |  | write something useful for field3 |
| [23:16] | byte2 |  | write something useful for field3 |
| [15:8] | byte1 |  | write something useful for field1 |
| [7:0] | byte0 |  | write something useful for field0 |

# reg1

Name

reg1

Address

0x1

Reset Value

0x00000001

Access

read-write

Description

write something useful for reg0

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:0] | field0 |  | write something useful for field0 |

# reg2

Name

reg2

Address

0x2

Reset Value

0x00000001

Access

read-write

Description

write something useful for reg0

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [5:4] | monkey2 | chimp=0, gorilla=1, phb=2 | which monkey |
| [3:2] | monkey | chimp=0, gorilla=1, phb=2 | which monkey |
| [1:1] | power2 |  | write something useful for field power2 |
| [0:0] | power |  | write something useful for field power |

# reg3

Name

reg3

Address

0x3

Reset Value

0x00000001

Access

read-write

Description

write something useful for reg3

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:0] | field0 |  | write something useful for field0 |

# reg4

Name

reg4

Address

0x4

Reset Value

0x0000000c

Access

read-write

Description

reg4 is a very useful register. It can take down the moon when configured correctly.

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:0] | reg4 |  |  |

# reg5

Name

reg5

Address

0x5

Access

read-write

Description

reg5 is as useful as reg4 but without a reset value defined.

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:0] | reg5 |  |  |

# reg6

Name

reg6

Address

0x6

Access

read-only

Description

reg6 is a read only register.

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [31:0] | reg6 |  |  |

# reg7

Name

reg7

Address

0x7

Reset Value

0x00000000

Access

read-write

Description

write something useful for reg7

|  |  |  |  |
| --- | --- | --- | --- |
| Bits | Field name | Type | Description |
| [19:16] | nibble2 |  | write something useful for field3 |
| [15:12] | unused1 |  | unused |
| [11:8] | nibble1 |  | write something useful for field3 |
| [7:4] | unused0 |  | unused |
| [3:0] | nibble0 |  | write something useful for field0 |